# ID 110269

Inadmissible value for time basis of velocity.
Description | The specified time velocity resolution (numerator) is out of range.
Response | Class | 3 | Abort!
Solution | Class | 7 | Correct parameter list of axis.
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [-]
P-AXIS-00206
Error type | 2, Error message by data transfer from parameter list into control device.