# ID 90011

Block memory for non-relevant channel blocks engaged.
Description | Non-relevant blocks are blocks without transaction information for the TRC. M functions are an example of non-relevant blocks: The number of consecutive non-relevant channel blocks is greater than the internal block memory reserved for them.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Modification of the NC-Program. Interrupt the sequence of non-relevant channel blocks without movement-information through a channel block with these movement-information.
Parameter | %1: | Upper limit value [-]
Number of the possible non-relevant blocks in sequence.
Error type | 1, Error message from NC program.