# ID 80000

Dead time exceeds maximum value.
Description | The dead time specified for the simulation drive is invalid. The parameter P-AXIS-00194 specifies this as a multiple of the cycle time of geometry processing.
Response | Class | 1 | Warning, reduce the dead time to the maximum permissible value
Solution | Class | 1 | Correct the dead time in the axis parameter see P-AXIS-00194
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Current value [-]
Specified value for the dead time see P-AXIS-00194
%3: | Upper limit value [-]
Maximum permissible value for dead time
Error type | -