# ID 110594

Invalid bit number for additional 'Ready for Power test'.
Description | Additional 'Ready for Power' test was enabled but the bit number configured in P-AXIS-00709 for this test is invalid. The smallest permissible value for P-AXIS-00709 is 0. Depending on the length of the configured telegram element used to transfer the additional ready for power test information, the maximum value of this parameter is:
Telegram element length | Maximum value for P-AXIS- 00709
2 | 15
4 | 31
This error message is also output if no value is configured for P-AXIS-00709.
Response | Class | 3 | Error message output, ready for power test is disabled.
Solution | Class | 1 | P-AXIS-00709 must have a permissible value assigned, or disable the ‘Ready for Power' test.
Parameter | %1: | Logical axis number [-]
%2: | Incorrect value [-]
Current value of P-AXIS-00709.
%3: | Limit value [-]
Limit value for P-AXIS-00709.
%4: | Corrected value [-]
Corrected value of P-AXIS-00709.
Error type | 2, Error message on data transfer of parameter lists to controller.