# ID 21101

SERCOS-Parameter: Date greater than max. value.
Description | SERCOS drive data blocks are transmitted during the cyclic data communication of the . These contain names, attribute, unit, maximum and minimum input value and the date. When this error occurs, the input value of the date is greater than the permissible maximum value of date.

More detailed informations you can get from the documentation of the drive manufacturer.

Response | Class | 3 | Abort NC program processing.
Solution | Class | 3 | Consult the documentation of the drive manufacturer.
Parameter | %1: | Current value [-]
Error message of the service channel
%2: | Identification number [-]
SERCOS ident number
Error type | 1, Error message from NC program.