# ID 150090

Illegal resolution of hand wheel in hand data.
Description | In the manual operation mode parameter data set, the value 0 has been parameterized for at least one of the parameters P-MANU-00005 or P-MANU-00006. These parameters together define a handwheels resolution.
Response | Class | 3 | Manual mode parameters are not taken over from CNC and start-up of CNC system stops.
Solution | Class | 6 | Correction of the values of P-MANU-00005 or P-MANU-00006.
Parameter | %1: | Current value [-]
Value of parameter P-MANU-00005 or P-MANU-00006.
%2: | Logical control element number [-]
Logical input device number of that handwheel with the incorrect parameter.
Error type | 2, Error message by data transfer from parameter list into control device.