# ID 110228

Logical axis number in axis parameter list and in command-PDU not equal.
Description | CNC gets an order to parametrize an axis with a data set from a given list. The message appears, because the number of the logical axis in the list isn’t the same as that of the axis.
Response | Class | 3 | Abort interpretation of the list.
Solution | Class | 7 | Check which list is to be used for parameterizing the axis. May be you have to change the number of the logical axis in the list or have to use another list.
Parameter | %1: | Current value [-]
Number of a logical axis. This number comes from the list that should be interpreted.
%2: | Expected value [-]
Number of logical axis, which should be parametrized with the values contained in list.
Error type | -