# ID 46057

No filename or filepath was assigned to input ParamAuto.
Description | An axis group is in operation mode Automatic mode. To start an NC program, a rising edge was applied to the "Start" input of the MCV_GrpOperationMode function block. To start the NC program, the file containing the NC program must be defined via the “ParamAuto” input at the time of the rising edge at the “Start” input. Assign the filename or absolute filepath for this file to the “ParamAuto” input as a character string.

An error is output since only an empty character string is applied to the “ParamMdi” input at the time of the rising edge at the “Start” input.

Response | Class | - | No job is sent to the motion controller.
Solution | Class | - | At the time of the rising flank at the “Start” input of the MCV_GrpOperationMode function block, assign a valid filename or absolute filepath to a file containing an NC program to the “ParamAuto” input.
Error type | -