# ID 70449

Feature bit set but P-0-4077 not configured.
Description | The process data element P-0-4077 belonging to feature bit was not configured in the cyclic process data.
Response | Class | 5 | Error message output, stop of axis, error is not resettable.
Solution | Class | 7 | Either configure P-0-4077 in the cyclic process data or reset the feature bit. Restart the controller.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Drive type [-]
Drive type P-AXIS-00020
%3: | Current value [-]
Value of the feature bit
%4: | Current value [-]
Status bit array of the commanded configured cyclic telegram.
Error type | -