# ID 40052

Value of SERCOS phase exceeds range 0..4.
Description | The value at the "Phase" input or output of a function block that allows access to the phase of a SERCOS ring does not correspond to the defined values for the phase of the SERCOS ring.
Response | Class | - | The job to read/write the phase of the SERCOS ring is dismissed.
Solution | Class | - | After correcting the value at input "Phase" start job again, if the value should be written. If the value of the phase of the SERCOS ring should be read , try to do it with another software tool.
Error type | -