# ID 70273

Different names for EtherCAT master process.
Description | Different names for the EtherCAT Master were specified for two or more axes under the realtime operation system INtime (see P-AXIS-00372). However, only one EtherCAT master process is supported by the controller.
Response | Class | 5 | Abortion of start-up
Solution | Class | 7 | Use identical process name P-AXIS-00372 for all axis
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Error value [-]
Specified process name, see P-AXIS-00372
%3: | Expected value [-]
Expected process name see P-AXIS-00372
Error type | -