# ID 110388

Maximum path distance for homing of gantry slave axis is less than 0.
Description | A value smaller than zero for P-AXIS-00284 was entered in the axis parameter list. The value is corrected automatically by adopting the set value.
Response | Class | 1 | The set value is re-used.
Solution | Class | 1 | Check value of P-AXIS-00284.
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis, see P-AXIS-00016
%2: | Current value [0.1 µm or 0.0001°]
Current set value, see P-AXIS-00284
%3: | Limit value [0.1 µm or 0.0001°]
Lower limit value for P-AXIS-00284 (0)
%4: | Corrected value [-]
Corrected value.
Error type | 2, Error message on data transfer of parameter lists to controller.