# ID 20037

#ACHSE is programmed without G200/G201/G202.
Description | The NC command #ACHSE[] was programmed but cannot be evaluated because G200/G201/G202 were not specified as well. Example: Wrong: N10 G00 X0 Y0 Z0 N20 #ACHSE[X]

N1000 M30

Correct:

N10 G00 X0 Y0 Z0

N20 G201 #ACHSE[X]

`N1000 M30`

Response | Class | 2 | Abort NC program processing..
Solution | Class | 3 | Check and modify NC program. Add G200 / G201 / G202.
Error type | 1, Error message from NC program.