# ID 50914

Online extension: inconsistent circle parameter.
Description | In die sinking technology with active equidistant calculation, a block parameter inconsistency occurred in a circular block. The equidistant calculation is defined by #TRACK CHAN ON[EXTEND=1 MAX_SCALE=6 MAX_EQUID=8]
Response | Class | 4 | Movement stop.
Solution | Class | 7 | Please contact the control manufacturer.
Error type | 1, Error message from NC program.