# ID 110040

Simulation drive: dead time exceeds maximum limit.
Description | The dead time for simulation drives is specified by P-AXIS-00194. The given value is invalid.
Response | Class | 1 | Warning and correction of parameter.
Solution | Class | 1 | Check and modify P-AXIS-00194 in the parameter list of the affected axis.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Error value [-]
Configured value of P-AXIS-00194
%3: | Limit value [-]
%4: | Corrected value [-]
P-AXIS-00194
Error type | 2, Error message by data transfer from parameter list into control device.