# ID 20680

Coordinate from forward transformation is out of data format.
Description | When a Cartesian transformation (#CS ON[...] or #ACS ON[...]) is selected, the program detects that an axis position exceeds the permissible value range after transformation.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check the machine axis positions before selection of the coordinate transformation. In the NC program, move to a smaller axis position before selecting this option.
Parameter | %1: | Error value [0.1 µm or 0.0001°]
%2: | Lower limit value [-]
%3: | Upper limit value [-]
%4: | Logical axis number [-]
Error type | 1, Error message from NC program.