# ID 50058

Measurement function is already selected (edge bending).
Description | It is not allowed to measure with G100 while edge bending G108 is still enabled. For detailed information on measurement function G100 and G108, see [PROG// Section: Measuring functions] [PROG// Section: Edge bending (G108)]
Response | Class | 4 | Movement stop.
Solution | Class | 6 | Check CNC program and measuring sequence, G100 and G108 are mutually exclusive.
Error type | 1, Error message from NC program.